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Properly fixed pin in the
masonry.
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Clean the hole with the
brush (xd).
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Insert screw of required
diameter into the plug
through fixture and tighten.
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Drilla hole to the required
diameter and depth for
rebar size being used.
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Insert UNO plug into hole
and tap home.





